Patricia Solvignon June 10, 2002

Oven Parameters

Menu Submenu Setting

Output Redirection S1.o1 Input Type RTD RTD Type 385.3 RTD Value 100 Alarm 1 Enabled Type Absolute Latched Latched Contact n.c. Setup Above Power On Enabled Low Value (anything) Hi Value 200 Alarm 2 Not Installed Loop Break Disabled Output 1 Self Disabled % Low 0000 % High 0095 Control Type PID Action Type Reverse Auto PID Disabled Adaptive Control Disabled Anti Integral Disabled Start PID Disabled Proportional Band 0010^∗ Reset Setup 0500^∗ Rate 0000^∗ Cycle Time 0001 Damping Factor 0001 Output 2 (any) (anything)

∗ On pheater.adl: enter → Prop. Band= 100; → Reset= 500 and → Rate=0

Menu Submenu Setting

Ramp & Soak Ramp Disabled Soak Disabled Analog Ouput Not Installed Communication Option Baud 9600 Parity no Data Bits 7bit Stop Bits 1bit Bus Format Checksum no Line Feed no Echo no Standard 232C Mode Command Separator Space Data Format Status yes Reading yes Peak no Valley no Unit yes ID no Address Setup (any) (anything) Transmit Time (any) (anything) Remote Setpoint Not installed

Comments: The PID parameters may change and will be updated in tlog. So look at the last tlog entry about PID parameters.