1. 24 drift chambers with two-cathode and wire readout operational at JLab.
2. Precise reconstruction of the 2D position of the avalanche around the wire.
3. Azimuthal extent of the avalanche estimated for an Ar/CO2 gas mixture.
4. Space charge effects within the same track observed by means of cluster counting.