# HALL B WORKER SAFETY AWARENESS TRAINING (SAF111)

###### *Purpose*

Familiarize users with safety hazards and protection systems in the Counting House and Hall.

###### *Training*

All users should take guided walkthrough covering the Hall B Counting House, labyrinth and Hall B using the latest update of the Emergency Response Guidelines (ERG) document for the hall.

For this, the user should contact the person responsible for the training,

Hall B/SAF111 -­­ Stepan Stepanyan (x-­­7196, stepanya@jlab.org)

Doug Tilles (cell:757 810-­­9576, mailto:tilles@jlab.org)

The guided training will, at a minimum, go over the likely hazards as well as the protection & emergency systems and procedures outlined in Appendix A of the ERG that one finds in the Counting House, personnel access stairs/tunnel and the hall. The JLab Skill Requirements List (SRL) tracking system (i.e. training) will be used to track the training status.

The SAF111 training does not have an expiration date. If however, the conditions of a hall are deemed to have changed sufficiently by the Division Safety Officer, the SAF111 training will be invalidated (forced to expire). The training tracking system will, like with any other training, notify all those affected so that they can make arrangements to take again the guided SAF111 training.

SAF111 training is required for unescorted access to the hall and to be able to take shifts in the Counting House – “escorting” of shift personnel is not allowed.

# Emergency Response Guidelines (ERG)

As part of the Experiment Readiness Review Process and Approval, every experiment is required to submit, in addition to the Conduct-­­of-­­Operations (COO), Experiment Safety Assessment Document (ESAD) and, Radiation Safety Assessment Document (RSAD), a document that summarizes the location of major hazards in the hall, the location of the various emergency systems as well as emergency procedures and egress routes during that experiment: the Emergency Response Guidelines (ERG) – this document. Shift personnel and anyone else wishing access to the hall during the duration of the experiment, must read and sign to indicate they have understood the COO, ESAD, RSAD and ERG of the experiment. Anyone feeling in doubt with the information contained in the ERG should contact the person responsible for the Hall

Worker Awareness Training and schedule guided refresher training.

###### *Purpose*

Familiarize users with safety hazards and protection systems in the Counting House and Hall.

###### *Prerequisites to access the halls without escort*

ES&H Orientation (SAF100)

Rad Worker I Training or equivalent (must have been issued a dosimeter by JLab) ODH training (SAF103)

General Access Radiological Work Permit [RWP] (SAF801kd) Hall B Worker Safety Awareness Training (SAF111)

###### *Reminder*

* **No one under 18 years may enter the halls**
* **No sandals or open toe shoes in any hall**
* **No shorts, long pants are required in the hall**
* **No food or drinking inside the halls**
* **Check postings at the entrance to the hall for special requirements** (e.g. hardhats are mandatory in Hall B and often required in the other halls). ***If in doubt, please contact the Hall Work Coordinator or his/her designee,***

Hall B -­­ D. Tilles [cell (757) 810-­­9576, [tilles@jlab.org](mailto:tilles@jlab.org)]

* Check that all work or test set ups follow the work controls indicated in the ESH&Q manual (<http://www.jlab.org/ehs/ehsmanual/index.html)> and on the supplemental Physics Division Work Planning Guidance ([http://www.jlab.org/div\_dept/physics\_division//work\_guidance\_final.pdf).](http://www.jlab.org/div_dept/physics_division/work_guidance_final.pdf)) **If in doubt, consult the Safety Warden of the area in which the work will take place, the Physics Division ESH&Q coordinator (B. Manzlak) or the Physics Division Safety Officer (P. Rossi).**

###### *The two-­­person rule (‘’Buddy Rule’’)*

Accessing the halls or performing work in the halls may require that personnel work on teams of at least two people. The two-­­person rule must be followed when entering Hall B or when performing a task in any of the halls that requires two-­­persons as indicated by the applicable general JLab safety rules or task OSP/TOSP. Examples of tasks that require two-­­persons would be operation of the hall crane, use of a man-­­lift, performing cryogenic, electrical or welding work**. Check postings at the entrance to the hall for special requirements. *If in doubt, please contact the Hall Work Coordinator or his/her designee.***

###### *Undergraduate Students in the Experimental Halls*

Regardless of hall or task, undergraduate students must follow the two-­­person rule during their first three-­­months at JLab. During that period, undergraduate students are allowed to work in the hall if (a) their work in the hall is always under the supervision of a hall-­­authorized ``buddy’’ (the ``buddy’’ can not be another undergraduate) and, (b) a permanent JLab staff member is cognizant of the work to be done, has supervisory responsibility for their work and approves the

``buddy’’.

# Appendix A













This appendix lists likely hazards, protection & emergency systems used and emergency procedures to be reviewed during the Hall Worker Awareness Training

### Hazards:

* Fire (electrical equipment, breaker panels, paper, trash, cables)
* Tripping and overhead hazards
* Falling hazards
* Elevated work
* High-­­pressure systems including low-­­conductivity water distribution
* Radiationhazards (beam-­­on, contaminated and activated areas)
* Loud noise hazards (thin vacuum windows)
* Flammable gasses
* Cryogenic (ODH and “cold-­­bite”)
* Magnets and magnetic fields
* Electrical
  + AC & DC (various voltages)
  + Magnet power supplies and their current distribution systems
  + High-­­Voltage supplies





Protection & Emergency systems and procedures:

* Signs and postings,
  + Radiation areas
  + Hearing protection requirements
  + Exit signs
  + Exit routes (evacuation plans)
  + Oxygen Deficiency Hazards
* Personnel Protection Requirements (e.g. hardhat, safety glasses, …)
* First Aid kit and Emergency Defibrillator
* Telephone locations with emergency numbers
* Fire
  + Detection systems (e.g. the Very Early Smoke Detection Apparatus [VESDA])
  + Alarm pull boxes
  + Fire alarm bells
  + Extinguishers and escape equipment (Hall B only)
  + Evacuation routes and muster points
* Electrical
  + Power shutoff switches
  + Circuit breaker panels
* Weather related hazards
  + Tornado emergency response
* Emergency lights
* Beam status, interlock and abort
  + Machine State Status Indicators,
  + Magenta/purple beacons,
  + Access doors to hall
  + Key interlocks
  + Run/Safe boxes
* Oxygen Deficiency Hazard condition detection
  + Sensors locations
  + Blue beacons & alarms locations
* Radiation Monitors (Controlled Area Radiation Monitors – CARMs)
* RadCon staging areas for equipment to be removed from hall
* Red beacons for hazards (e.g. energized magnets and cranes)
* Yellow beacons for warning or caution (e.g. energized lasers, forklifts)
* Cabinets for storing flammable materials
* Lockout/Tagout Stations
* Eye wash stations



|  |  |  |
| --- | --- | --- |
| **FOR HALL WORKER AWARENESS TRAINING ONLY**  f  • \_ I  Uptm'1i!! \_]  I  ...,....;tlm  I  -/"' ' ' '"'" ' ' p ljil- rl-- l±llH  I  I I UP  I I  I I  'i \"  @] II **mt** -  DOWNSTREAM ALCOVE I I UPSTREAM  '1I **0** I ALCOVE  I  I  I I  e t ;It1fm  I  =l!il- \_J  UP  **Ci** |  | |
|  | EXPERIMENTAL HALL B BUILDING 94,FLOOR 0 EMERGENCY PLAN |
|  | I 1INCASE OFFIRE  STAYCALW WALK,00NOTRUN  ACTIVATE NEARESTPULL BOX,  FOLLOW ARROWS INDIAGRAM,& MEET AT MUSTER POINT  INCASE OF SEVERE WIND:  IF A TORNADO WARNING IS ISSUED BY THENATIONAL WEATHERSERVICE,AND JLAB ISWITHINTHE WARNINGAREA, MOVE QUICKLY *TO* ONEOFTHE DESIGNATEDSEVEREWIND 'TAKE  CO.V.ER"AREAS. LEGEND  **t** EGRESS PATH  •FIREEXTINGUISHER  FIRE ALARM PULL STATION  **0** SEVEREWIND"TAKECOVER" AREA  **Ci** MUSTERPOINT  TELEPHONE  @ EMERGENCYEXITSWITCH  [ill§] RUN/SAFEBOX  ICPD I CRANE POWERDISCONNECT  ISRF I SMOKEREMOVALFAN  IEPO I EMERGENCYPOWEROFF  & MAGNETIC FIELD  illELECTRONICS*I*POWER  0 EYE WASH |

**FOR HALL WORKER AWARENESS TRA INING ONLY**




EXPERIMENTAL HALL B BUILDING 94,FLOOR 1 EMERGENCY PLAN

INCASE OFFIRE:

STAY CALM WALK,DO NOT RUN

ACTIVATE NEAREST PULL BOX, FOLLOW ARROWS INDIAGRAM,& MEETAT MUSTER POINT

I , -- , 1 DOWNSTREAM ALCOVE



&

IN CASE OFSEVERE WIND:

IFA TORNADO WARNING IS ISSUED BY THE NATIONAL WEATHER SERVICE, AND JLABIS WITHINTHE WARNINGAREA, MOVEQUICKLY TO ONE OF THE DESIGNATED SEVERE WIND "TAKE

CO.VE.R" AREEGARSE.SS PATH

LEGEND

•

'

FIREALARMPULLSTATION FIRE EXTINGUISHER

**g** SEVEREWIND"TAKECOVER"

AREA

MUSTER POINT

TELEPHONE

@ EMERGENCYEXITSWITCH

[E!§J RUN/SAFEBOX

ICPD I CRANE POWER DISCONNECT

ISRF I SMOKE REMOVAL FAN

IEPO I EMERGENCY POWER OFF

& MAGNETIC FIELD

ill

|  |  |  |
| --- | --- | --- |
|  | | |
|  | | & NNEL |
|  | |
| UPSTREAM ALCOVE |  |
| TU |

**FOR HALL WORKER AWARENESS TRAINING ONLY**

EXPERIMENTAL HALL B BUILDING94,FLOOR2 EMERGENCY PLAN

INCASEOFFIRE:

STAY CALM WALK,DO NOT RUN

ACTIVATENEAREST PULLBOX, FOLLOWARROWS INDIAGRAM,& MEET AT MUSTER POINT





### *\_J* -r=--=--=--=--=--=--=-

t

\_ \_J

IN CASE OF SEVEREWIND:

IF A TORNADO WARNING IS ISSUEDBY THE NATIONAL WEATHER SERVICE, AND JLABISWITHINTHE WARNINGAREA, MOVEQUICKLY TO ONEOF THE DESIGNATED SEVERE WIND"TAKE



..EAS.

LE GEND COVER" AR

I L \_ \_ \_ \_ \_

L - \_,

EGRESSPATH

•**r**

FIRE EXTINGUISHER

FIRE ALARM PULL STATION

**g** SEVEREWIND"TAK ECOVER" AREA



MUSTER POINT

TELEPHONE

® EMERGENCY EXIT SWITCH RUN/SAFE BOX

CRANE POWER DISCONNECT



SMOKE REMOVAL FAN EMERGENCY POWER OFF

& MAGNETIC FIELD

&ELECTRONICS*I*POWER

0 EYEWASH

## FOR HALL WORKER AWARENESS TRAIN I NG ONLY



EXPERIMENTAL HALL B BUILDING 94, FLOOR 3 EMERGENCY PLAN

INCASE OF FIRE:

STAY CALM WALK,DO NOT RUN

ACTIVATENEARESTPULL BOX, FOLLOW ARROWS INDIAGRAM,& MEET AT MUSTER POINT

J1--- -

\_ \_J

-,

T

I I

\_ \_ \_ \_ \_ \_ \_ \_ \_ \_ \_ J I I

-----------*---1\ \_s =*

INCASEOFSEVEREWIND:

IFA TORNADO WARNING ISISSUED BY THE NATIONAL WEATHER SERVICE, AND JLAB IS WITHIN THE WARNING AREA, MOVE QUICKLY TO ONEOF THE DESIGNATED SEVERE WIND "TAKE COVER" AREAS.

.

LEGEND

I L \_ \_ \_ \_ \_ \_

t

L \_ \_ \_ \_ \_ \_ \_

**G**•'

EGRESS PATH FIRE EXTINGUISHER

FIREALARM PULL STATION

SEVERE WIND "TAKE COVER" AREA

MUSTER POINT

TELEPHONE

@ EMERGENCY EXIT SWITCH

[iii[] RUN/SAFEBOX

ICPDI CRANEPOWER DISCONNECT

ISRF I SMOKE REMOVAL FAN

IEPO I EMERGENCY POWER OFF

&MAGNETICFIELD

illELECTRONICSIPOWER

0 EYEWASH

***Emergen*f a**



**f faa**

***cy Response Procedures***

**Important information**

#### DIAL

**9-911 or 911**

Both numbers will connect you to:

**City of Newport News' Emergency Dispatch Center**

If dialed from a land-line phone the following are automatically alerted:

* JLab Security
* Occupational Medicine
* Other key JLab Responders.

If dialed from a cell phone you will also need to call:

**JLab Security @ 269-5822**

**EVENT ACTION 1 ACTION 2 ACTION 3**

**Injury or acute illness**

**Call 9-911 or 911**

* + Stay with the victim while awaiting emergency responders
  + Do not move the victim unless they are endangered at location
  + Administer first aid/CPR if willing and trained
  + Avoid contact with other's blood

If possible send someone to flag down the ambulance

**Direct minor injuries to Occupational Medicine (Support Service Center, Bldg 28, Room 22) during regular business hours.**

Most buildings have one or more first-aid cabinets and AEDs for your convenience. There are pamphlets at these locations to assist you.

**Await "All-Clear**

**Sound Alarm** (use the nearest pull box)

**Evacuate to Muster**

**Evacuate to Muster Point** (refer to the evacuation map for your location)

**Notification"**

From Fire Protection Engineer or Building Drill Coordinator before re-entry.

**Fire Alarm**

**Point**

(refer to the evacuation map for your location)

**Await "All-Clear Notification"**

From Fire Protection Engineer or Building Drill Coordinator before re- entry.

**Unexplained Odor of Natural Gas**

**Sound Alarm** (use the nearest pull box)

**Evacuateto MusterPoint** (refer to the evacuation map for your location)

**Call JLab Security**

@ 269-5822

**Severe Weather Warning**

(via weather alert radio, outdoor siren, or other official source)

**Immediately:**

* + - **Pass the Word**
    - **Taking Cover**

(refer to the evacuation map for your location)

**Protect Yourself from** If there are

**Earthquake Do Not Evacuate Building**

**Write Down:**

* + - * Any demands/instructions

**Falling Objects**

(get under a desk or table)

**Call JLab Security**

@ 269-5822

injuries or damage

**Call JLab Security**

@ 269-5822

**Bomb Threat**

**OIL SPILL**

* Caller's number if available
* Vocal characteristics
* Any other relevant details to identify the caller

**Call JLab Security**

@ 269-5822

**or**

**Sound Alarm** (use the nearest pull box)

**Cordon Off Area** Keep people away

**Evacuate to Muster Point**

(refer to the evacuation map for your location)

**Wait**

for trained and equipped staff to control and contain the spill

**ODH Alarm**

or visible plume

**Evacuateto MusterPoint** (refer to Supervisor's instructions for your location)

**Call JLab Security**

@ 269-5822

**Call Crew Chief**

@ 269-7045

**Radiation Alarm**

**Hit**

"Push to Safe"

**RED**

Button

**Evacuateto MusterPoint** (refer to the evacuation map for your location)

**Call Crew Chief**

@ 269-7045

**Automobile Accident** If anyone is injured.

**Call 9-911 or 911**

**Call JLab Security**

@ 269-5822

**Call Facilities Management**

@ 269-7400

**Intruders, Threatening or Abusive Behavior**

other unauthorized conduct

**Trouble Indication** audible alert in fire alarm panel

Requests

to **Serve Summons**

or other legal documents Requests for

**Call JLab Security**

@ 269-5822

**Ensure Your Personal Safety!**

**Run, Hide, Fight**

(See ES&H Manual Chapter 3510-T5 Active Threat Emergency Procedure and HR Workplace Harassment and Violence Policy)












**Call Facilities Management**

@ 269-7400

**Call JLab Security**

@ 269-5822

**Personal Information**



about JLab staff or visitors

Requests for passwords or other **Computer-Access** information

Requests for **JLab News, Status**, or other information

Rev. 04/2014

You are not authorized to provide any information about JLab staff members

**Refer Requestor to Human Resource Representative @ 269-7068**

You are not authorized to provide any information about computer accounts, passwords, user names, and so forth

**Refer Requestor to Computer Center Help Desk @ 269-7155**

You are not authorized to provide any information regarding JLab status or conditions

**Refer Requestor to JLab Public Information Office @ 269-7689**

[Click to Update](https://misportal.jlab.org/mis/training/online_courses/completeClass.cfm?classId=88451)